Cause:
- the signal at the digital input parameterized with the controller enable function "RF" was switched off during travel
Remedial action:
- check the activation and control of "RF" signal
- check the safety circuit