Cause:
- no change is made to the remaining distance during the travel
Remedial action:
- check the elevator controller compatibility with DCP specification
- check the absolute value encoder for the right determination of the remaining distance