Cause:
- when using a power recuperation unit in combination with a braking resistor, the temperature monitoring of the braking resistor is not parameterized
Remedial action:
- parameterize a digital input (preferably "X_BR4") with the "PFU_BR" function in the "Control system" menu