Cause:
- during travel at a speed greater than 10 cm/s the position in shaft does not change within 200 ms (CAN position mode)
Remedial action:
- check the CAN absolute value encoder in the shaft
- check the traction capability of the drive (traction sheave)