Cause:
- at the start of the travel, the measured motor temperature is too high
Remedial action:
- check the connection of the temperature sensor (motor) at terminal X-MT
- check whether the motor has overheated
- remove the cause of overheating of the motor (reduce the duty cycle, check the load conditions of the system, check the motor parameters, adjust the absolute encoder for synchronous machines, cool the motor down...)