Cause:
- error during communication with the absolute value  encoder (motor)
Remedial action:
- check the cable of the absolute value encoder
- check the type of the connected absolute value encoder
- check EMC-compliant installation of the system (motor and braking resistor cable shielding)
- for further information see INFO menu "Encoder"