Cause:
- U/f operation (sensorless) in combination with the control type CAN position mode or DCP04 is not allowed
Remedial action:
- change the control mode in the elevator control to CAN velocity mode
- change the "CONFIG" parameter in the "Control system" menu to DCP03