Cause:
- despite deactivated output "MB", a movement of the drive is detected
Remedial action:
- check the motor brake for sufficient braking torque
- check brake release time
- the motor brake must be controlled simultaneously with the switching of the relay with the output function "MB"