Cause:
- during a travel with the reference speed V_Z (readjustment), the measured speed was 10 % higher than the specified target speed value
Remedial action:
- check the parameters set in the "Motor nameplate" menu
- check the parameters "SPD_KP" and "SPD_TI" in the "Controller" menu