Cause:
- in the "Encoder & BC" menu, the setting of the "ENC_INC" parameter does not match the resolution of the absolute value encoder (motor)
Remedial action:
- set "ENC_INC" to the correct resolution
- for further information see INFO menu "Encoder"