Cause:
- the motor current exceeds the value "I_MAX" for the time "T_MAX" in the menu "Monitoring"
Remedial action:
- check the motor data in "Motor nameplate" menu
- check the weight compensation
- check the brake activation and functioning
- check the dimensioning of the installation