Cause:
- during decelerating, the transmitted distance-to-go was increased (DCP04) or a new target position was specified (CAN)
Remedial action:
- check the absolute value encoder for the right determination of the remaining distance
- check the elevator controller compatibility with DCP specification
- in info menu Bus Info 3 check the ratio between distances measured by the absolute encoder (shaft) and motor encoder (line 4)