Cause:
- by travel start, the signals STO_A and STO_B are missing at the connection terminal X-STO
Remedial action:
- check the wiring
- check the supply voltage of the relays
- check the control voltage of the STO signals
- when using the ZAsbc4: Reset ZAsbc4 by switching it off and on again