Cause:
- the temperature of the power section is too high at the start of the travel
Remedial action:
- check the functioning of the cooling fan
- check the ambient temperature
- eliminate the cause of overheating (reduce the duty cycle, check the load conditions of the system, check the motor parameters, adjust the absolute value encoder for synchronous machines, ...)