Cause:
- the communication between the motor management processor (MOP) and the application processor (APP) was interrupted
Remedial action:
- check the EMC-compliant installation of the system (shielding, etc.)
- in case of permanent occurrence: please contact ZIEHL-ABEGG customer service