Cause:
- with the quick start function activated, the drive moves by more than 7 mm while the speed is held at 0 m/s
Remedial action:
- check the motor data in the "Motor nameplate" menu
- check the parameter "SPD_KP" in the "Controller" menu
- check the motor connection (U-U; V-V; W-W)