Cause:
- the board for the monitoring of the motor temperature is not recognized
Remedial action:
- check the correct mounting/connection of the circuit board
- set the parameter "P1P2" to "Off" in the "Monitoring" menu
- replace the circuit board