Cause:
- the absolute value encoder (motor) was not detected at the start of the travel
Remedial action:
- check the connection of the absolute value encoder 
- check the setting of the "ENC_TYP" parameter in the "Encoder & BC" menu
- for further information see the INFO menu "Encoder"