Cause:
- on an emergency stop the brake release monitoring contacts do not have a time lag of at least 50ms on a BD132
Remedial action:
- check the brake release monitoring wiring of the motor (install the free-wheeling diode)