Cause:
- at the end of the travel, after the time "T_SDLY" in the "Monitoring" menu has elapsed, a signal is still present at the inputs STO_A and STO_B
Remedial action:
- check the activation of the STO inputs
- adjust the time during which the STO inputs are controlled on the elevator control system