Cause:
- the communication between the motor management processor (MOP) and the application processor (APP) is interrupted at standstill
Remedial action:
- in case of permanent occurrence: please contact the ZIEHL-ABEGG customer service
- for sporadic occurrence: check the EMC-compliant installation of the system (shielding, etc.)