Cause:
- if motor temperature monitoring "P1P2 = PTC" is set in the "Monitoring" menu, the measured resistance at terminal "X-MT" is less than 20 Ohm
Remedial action:
- check the motor temperature monitoring connection 
- check the parameter "P1P2" in the "Monitoring" menu