Cause:
- the state of the signals STO_A and STO_B was differing for longer than 120 ms
Remedial action:
- check the activation of the STO inputs
- check the switching function of the relays
- check the control of the coupling relays