Cause:
- the monitoring contact of the recuperation unit (input "BC") opens during ZAdyn operation or is not closed during start-up
Remedial action:
- check the error display of the recuperation unit
- check the connection of the fault signal relay of the recuperation unit