Cause: 
- error message of the ZArec, the signal at the digital input parameterized with "ZR_RDY" drops out during the travel
Remedial action:
- use the ZArec display to check whether there is an error on the ZArec
- for sporadic occurrence: check the EMC-compliant installation of the system (shielding, etc.)