Cause:
- the brake monitoring system has reacted during travel
a) error at the end of the travel in the event of a brief interruption
b) travel abort in case of an interruption longer than 500 ms
Remedial action:
- check the correct functioning of the monitoring contacts
- check the brake activation and control
- check the supply voltage of the brakes