Cause:
- overcurrent at standstill
Remedial action:
- check the wiring of the brake chopper (if present)
- check the EMC-compliant installation of the system (shielding, etc.)
- in case of permanent occurrence: please contact ZIEHL-ABEGG customer service