Cause:
- a magnet of the DISCcontrol positioning system was not detected at the expected position
Remedial action:
- attach magnet to correct position
- glue on any dropped/missing magnets
- set the hall sensor to the correct distance
- check the backlash of the traction sheave bearings