Cause:
- a phase failure occurs during a motor mode travel and a reset is triggered. No error is generated during generator operation
Remedial action:
- check the 3 phases of the supply voltage (measure L1, L2, L3 to PE)