Cause:
- no communication takes place between the application processor and the motor management processor during start-up
Remedial action:
- in case of sporadic occurrence: Check the installation to be EMC-compliant (shielding, etc.)
- in case of permanent occurrence: please contact ZIEHL-ABEGG Customer Service