Cause:
- when using a ZArec4C recuperation unit, the functions "ZR_RDY" or "ZR_EN" were not parameterized
Remedial action:
- parameterize a digital input with the function "ZR_RDY" in the menu "Control system"
- parameterize a digital output with the function "ZR_EN" in the "Control system" menu