Cause:
- the motor test current was not reached at the start of the travel
Remedial action:
- check the motor connection and motor cable
- consult the ZIEHL-ABEGG Customer Service for further information