Cause:
- at the end of the travel, the motor contactors are not yet recognised as open after the time "T_CDLY" in the "Monitoring" menu has elapsed
Remedial action:
- check the wiring of the contactor monitoring system
- check the contactor activation and control
- check the contactors for functioning