Cause:
- the travel was aborted due to a CO interruption and the drive commands of the control remain active
Remedial action:
- check the safety circuit
- check the contactor activation
- check the evaluation of the ZAdyn output signals by the elevator controller