Cause:
- no signals are detected from the encoder (motor)
Remedial action:
- check whether the brake opens
- check the motor data
- check the motor connection (U-U, V-V, W-W)
- increase the parameter "SPD_KP" in the "Controller" menu