Cause:
- if brake release monitoring is active, at least one brake is detected as open before the start of travel
Remedial action:
- in the "Monitoring" menu, check the parameter "BR" for setting of the correct number and switching logic (NO / NC) of the monitoring contacts
- check the correct connection of the monitoring contacts
- check the functioning of the monitoring contacts