Cause:
- the motor temperature has exceeded the permissible limit during travel
Remedial action:
- check the parameters set in the "Motor nameplate" menu
- In the "Mot" info menu, check the motor current during constant travel (empty car downwards). The displayed motor current should not exceed the rated current of the motor. For asynchronous motors, carry out an automatic identification of the motor parameters if necessary (see parameter "ASM_ID" in the "Motor nameplate" menu).
- check the motor duty cycle (display in info menu "Power1", value "ED")
- for synchronous motors, check encoder offset of encoder
- check the brake release and monitoring