Cause:
- when the frequency inverter is switched on, the monitoring contact of the recuperation unit is not closed
Remedial action:
- check the recuperation unit for fault-free operation
- check the rotary field of the mains connection of the recuperation unit
- check the connection of the function monitoring of the recuperation unit to the digital input "BC"
- switch ZAdyn off and on again