Cause:
- the absolute value encoder (motor) transmits a warning indicating an imminent failure
Remedial action:
- the absolute value encoder must be replaced as quickly as possible
- temporarily, one of the parameters "MASKx" in the "Monitoring" menu can be set to 335 in order to mask the error