Cause:
- internal device error, the pulse width modulation was switched off
Remedial action:
- check the encoder connection
- in case of permanent appearance: please contact ZIEHL-ABEGG Customer Service
- for sporadic occurrence: check the EMC-compliant installation of the system (shielding, etc.)