Cause:
- overtemperature at power section
Remedial action:
- check the functioning of the cooling fan 
- check the ambient temperature 
- eliminate the cause for overheating (reduce the duty cycle, check the load conditions of system, check the motor parameters, adjust the absolute value encoder in case of synchronous machines, ...)