Cause:
- the motor shaft has turned during the encoder calibration with the brake closed
Remedial action:
- check if the brake was disconnected before starting the encoder calibration. The brake must not be opened during the calibration