Cause:
- the actual speed is greater than 105 % of the rated speed V*
Remedial action:
- check / increase the parameter "SPD_KP" in the "Controller" menu
- check the motor data in the "Motor nameplate" menu