Cause:
- the calculated power loss of the braking resistor exceeds the rated power by 25 %
Remedial action:
- check the parameter "BC_TYP" in the "Encoder & BC" menu
- if "BC_TYP" = "BRxx" check the parameters "R_BR" and "P_BR" in the "Encoder & BC" menu
- eliminate cause for overloading the resistor (reduce duty cycle, check load conditions of the system...)