Cause:
- the reference direction has been changed during a travel
Remedial action:
- check the control of the driving directions
- for sporadic occurrence: check the EMC-compliant installation of the system (shielding, etc.)