Cause:
- The "controlled emergency stop" function is already active at the start of the travel
Remedial action:
- check the setting of the digital inputs in the "Control system" menu
- check the activation and wiring of the input with the "/FastStp" function