Cause:
- Collective fault caused by an STO interruption (fault triggered within T_STO)
Remedial action:
- check the safety circuit
- check the activation of the STO inputs
- check the supply voltage of the relays 
- check the control voltage of the STO signals