Cause:
- Additional information 1: At the start of the travel, the brake control is not ready to operate
- Additional information 2: At the end of the travel, the brake control is still ready to operate
Remedy:
- For devices not equal to MDxxBR, switch off the input function "51:MD_BM_Fb"
- Check the safety chain, 230VAC must be present between N_SC and L_SC when starting
- Parameter "f_O3" must be set to "MotContact"
- Consult the ZIEHL-ABEGG Customer Service for further information