Cause:
- if mains voltage is present, the external 24 VDC power supply of the processor board (CU) exceeds the internal power supply by 1 VDC
Remedial action:
- remove the external 24 VDC power supply
- decrease the voltage of the external 24 VDC power supply