Cause:
- an overcurrent was detected at the output for the braking resistor
Remedial action:
- check the brake resistor connection for short-circuit and ground fault
- check the type of braking resistor used (see the operating instructions chapter "Brake resistor allocation")